University of Warwick                                             Substance Information Note 001

	Substance
	Aerosol Lubricating Oils
(e.g. WD40; AC90; 3-in-One etc.)
	UN No:  1950
Transport Cat: 2
	University Hazard Classification
	High

	Activity
	Lubricating metal components using spray oils


	Handling Requirements e.g. fume hood, MSC, glove type etc.
	This substance must only be used in a well-ventilated area or appropriate general extraction so that users do not breathe in vapours. Take measures against electrostatic charging as appropriate.  Workplace Exposure Limit (WEL) of the total hydrocarbon solvent content of the mixture (RCP method according to EH40) is 800mg/m3 (long term exposure 8h TWA). Respiratory protective equipment (RPE) is not normally required, if needed it must be face-fitted and meet EN 14387 standard (filter A2P2).   



	Laboratory Info
	 Appropriate to the department (Lab number and containment level where appropriate) 
	Additional Information
	Prolonged contact can cause dermatitis. Any changes in health status, which may be due to the use of this substance, must be reported to Occupational Health as soon as possible. 

In case of fire the following can develop: oxides of carbon, oxides of nitrogen, toxic pyrolysis products, may explode when heated, explosive vapour/air mixture.
	Hazard Statements
H222
H229
H304
H336
EUH066

	

Highly flammable aerosol

Pressurised container
May burst if heated	

Irritating to the Eyes and Skin

Prolonged or repeated contact causes skin irritation and may cause dermatitis.

	327025132080
High concentrations of vapour

Do not breathe vapours, will cause drowsiness, sickness and headaches 	339090122555
Harmful if swallowed

May cause sickness and drowsiness
	

	Handling Precautions


Follow advice given in the section “Good Hygiene Practice”

Always follow manufacturer’s instructions
	
	

Avoid skin contact.  Wear a long sleeved protective garment or overalls are advised 

Wear impervious gloves (EN 374) if prolonged skin contact cannot be avoided.

Use barrier creams and hand cleansers
	286385156845 




Wear safety goggles (EN166) if risk of splashing.

Do not direct spray at self or others.
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Always wash hands thoroughly after using this substance. 
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Do not smoke.
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Do not use near naked flame or other heat source.  




	Storage & Transport
	Store in a flammable cupboard away from sources of heat or ignition. 
Store in a well-ventilated place. 
Do NOT store with oxidising agents. 
Protect from frost, direct sunlight and temperatures over 50°C.  
Must not be stored in gangways or stair wells. 
Transport upright to prevent damage to spray nozzle.
	Spillage and Waste Disposal
	Spills: - Ensure sufficient supply of air. Take any leaking aerosols into open air or well-ventilated area away from sources of ignition and allow to empty completely.  Do not puncture or incinerate, even when empty.  Prevent surface and ground water infiltration as well as ground penetration. Prevent penetration into drains, cellars, working pits or any other places where accumulation could be potentially hazardous.  
Waste: - Collect in plastic bags and disposed of as hazardous waste in line with departmental procedures.  
	First Aid

[image: ]
	EYES:   Rinse immediately with clean running water for at least 15 minutes.  Remove contact lenses if applicable. Seek medical advice.

	
	SKIN:   Remove contaminated clothing, wash skin thoroughly with soap and water.  Do not use solvents. Seek medical attention if significant skin contamination has occurred.

	
	INHALATION:    Remove to fresh air and advise rest.  Seek medical advice if casualty is having difficulty in breathing.

	
	INGESTION:    If conscious, give casualty one pint of water.  DO NOT INDUCE VOMITING. Danger of aspiration. Seek medical attention urgently 
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