University of Warwick                                             Substance Information Note 040

	Substance
	DIESEL 

	UN No:  1202
Class Code: F1
Transport Cat: 3
	University Hazard Classification
	High

	Activity
	Dispensing into tractors, agricultural vehicles and generators etc.

	Handling Requirements e.g. fume hood, MSC, glove type etc.
	Diesel dispensing must only be carried out in well-ventilated areas or outdoors as it can release vapours that can readily form flammable mixtures. 
Smoking is strictly prohibited. 
Wash skin thoroughly after handling. 


	Laboratory Info
	Use only outdoors or in well-ventilated areas
	Additional Information
	Only trained individuals must dispense diesel fuel.
A responsible person must be nominated for ordering and organising deliveries.
A strict log of dispensed quantities of diesel MUST be maintained at all times.
Diesel store is locked at all times.
Workers handling diesel may be at risk of dermatitis and skin drying. They should regularly check their skin condition to ensure no noticeable changes have occurred 
Any change in health status you think may be related to using these products must be reported to your supervisor/line manager immediately and an Occupational Health referral made.  
	Hazard Statements
H226
H304
H315 
H332 
H351 
H373 
H411

	2927357302500
Flammable liquid and vapour

Keep away from hot surfaces, heat, sparks, open flames and other ignition sources  	3450857302500  



Causes skin irritation. 

Harmful if inhaled.
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May be fatal if swallowed and enters airways. 

Suspected of causing cancer.

May cause damage to organs through prolonged or repeated exposure (bone marrow, liver, and thymus).
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Toxic to aquatic life with long lasting effects

	

	Handling Precautions
P210 
P260 
P273 
P280 
P301 + P310 
P331 
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Chemical resistance gloves to EN 374 – must cover wrist



	34127465837

Wear long-sleeved protective overalls.

Contaminated clothing should be changed and not worn again until thoroughly washed.	[image: ]Wear goggles (EN166) where there is a risk of splashing.

	Insert appropriate safety symbols
	Storage & Transport
	Storage is in an enclosed tank within the Boiler House and dispensed via an approved metered nozzle housed on an exterior wall of the building in a secluded cupboard with a key entry system.  
Red diesel (gas oil) is dispensed directly into the tractor / agricultural vehicle tanks by approved operators in Horticultural Services team. This occurs in an open air environment and therefore maximum ventilation available.
Use explosion-proof electrical, ventilating and lighting equipment.
Use non-sparking tools
Take action to prevent static discharge
	Spillage and Waste Disposal
	Minor spillages on sealed ground: 
Eliminate all sources of ignition in immediate area. Use an absorbent spill kit available and follow local procedures. 
Place all waste in black plastic bin liners and carefully transfer to contaminated waste bin for approved supplier to dispose of appropriately. 
Land Spill: 
Eliminate all ignition sources (no smoking, flares, sparks or flames in immediate area). 
Stop leak if you can do so without risk. 
All equipment used when handling the product must be grounded. 
Do not touch or walk through spilled material.
Protect entry into waterways, drains, basements or confined areas using spill control booms. 
Absorb the spillage with absorbent material and non-sparking tools and transfer into waste containers. 
Water spray may reduce vapour, but may not prevent ignition in enclosed spaces.
Notification: In the event of a major spill or accidental release, notify the H&S team immediately who will contact the relevant authorities in accordance with all applicable regulations.
	First Aid
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	EYES:   Use one bottle of Diphoterine® per eye as per manufacturer’s instructions. If Diphoterine® is not available flush thoroughly with clean water for at least 10 minutes. Seek medical attention.

	
	SKIN:  If skin surface is damaged apply a clean dressing and seek medical attention. If skin surface ins not damaged, wash affected areas thoroughly with soap and water.   If irritation or redness develops seek medical attention 

	
	INHALATION:   If respiratory symptoms or other symptoms of exposure develop, move victim away from source of exposure and into fresh air in a position comfortable for breathing. If symptoms persist, seek immediate medical attention. If victim is not breathing, clear airway and immediately begin artificial respiration. Seek immediate medical attention..

	
	INGESTION:    Seek immediate medical attention. Do not induce vomiting.  If ingested, material may be aspirated into the lungs and cause chemical pneumonitis. Treat appropriately.
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