**Procedure for gas cylinder selection and use**

Select desired gas from stores or gas storage/cylinder racking.

Select suitable trolley

Fit cylinder restraints [chain/strap] to secure.

Use trolley to return cylinder to empties rack /stillage/stores. Secure.

Use

When **EMPTY**

Disconnect. Remove the **cylinder tag** from the hook/tag rack and place back on cylinder neck/shoulder.

Place **correct** **cylinder tag** on cylinder neck/shoulder

Attach cylinder to trolley.

Return **cylinder tag** to either a new full cylinder of correct type, or to tag rack.

Connect - check connections - open all delivery and service valves slowly – adjust and set regulator pressures.

Deliver to place of use.

Place **cylinder tag** on local hook or tag rack