

                      INSTRUMENT CONTROL PARAMETERS:    Instrument #1
                      -----------------------------------------------

   C:\MSDCHEM\1\URINE\100224 Urine 37.m

Control Information
------- -----------

Sample Inlet      :  Other/None
Injection Source  :  External Device

                                MS ACQUISITION PARAMETERS


General Information
------- -----------

Tune File                : atune.u
Acquistion Mode          : Scan
Run Length               : 0.75 min


MS Information
-- -----------

Solvent Delay            : 0.45 min

EM Absolute              : False
EM Offset                : 0
Resulting EM Voltage     : 2094.1

[Scan Parameters]

Low Mass                 : 10.0
High Mass                : 550.0
Threshold                : 150
Sample #                 : 2       A/D Samples    4
Plot 2 low mass          : 10.0
Plot 2 high mass         : 550.0

[MSZones]

MS Quad                  : 150 C   maximum 200 C
MS Source                : 230 C   maximum 250 C


                             END OF MS ACQUISITION PARAMETERS


                              TUNE PARAMETERS for SN:  
                        -----------------------------

 EMISSION    :      34.610
 ENERGY      :      69.922
 REPELLER    :      16.385
 IONFOCUS    :      78.769
 ENTRANCE_LE :      16.500
 EMVOLTS     :    2094.118
 AMUGAIN     :    1659.000
 AMUOFFSET   :     131.000
 FILAMENT    :       1.000
 DCPOLARITY  :       1.000
 ENTLENSOFFS :      17.067
 MASSGAIN    :    -395.000   
 MASSOFFSET  :     -10.000   


                           END OF TUNE PARAMETERS
                      ------------------------------------



                           END OF INSTRUMENT CONTROL PARAMETERS
                           ------------------------------------

